	S3.2 VHF MICROPHONE SYSTEMS


	

	THE SYSTEM

Giving unparallelled VHF clarity, the new S3.2 combines many of the features of the S3500 in a single frequency system.

The S3.2 system is available in hand held, lapel and headworn microphone versions as well as a dedicated guitar pack and incorporates the latest PLL Synthesised Tuning Technology.

Available on all DTI approved frequencies, the new S3.2 has a host of additional features including LEDs showing Power On, AF Peak level, RF Level and Diversity Channel A or B. In addition, the diversity operation receivers have front mounted telescopic antennae and variable gain jack plug output. The handheld version is also fitted with an Audio-Technica capsule and the guitar pack has a standard quarter inch jack plug. With transmitter battery life in excess of ten hours, the S3.2 is certain to give the performance of a lifetime. 


	THE RANGE

S3.2L: beltpack system
S3.2LM: as S3.2L but with TS259 lapel microphone
S3.2CHM: as S3.2L but with TS33 headband microphone
S3.2LHM: as S3.2L but with TS912 headband microphone
S3.2WHM: as S3.2L but with TS44 headband microphone
S3.2M: handheld system
All S3.2 systems come complete in a carrying case and are supplied with all necessary antenna, power supply and alkaline battery



	
	TECHNICAL SPECIFICATIONS
 

S3.2RX RECEIVER
RF Frequency Range: 170-220MHz (subject to UK licensing requirements)

Audio Frequency Response: 30Hz-18kHz (-3dB)

Noise Reduction: Complementary variable ratio compression/expansion with pre-emphasis/de=emphasis

Dynamic Range: >110dBA

Dimensions: 212 x 100 x 30mm

Weight: 490g

 

S3.2LTX TRANSMITTER
10 hour battery life (9v Alkaline Battery)

Single Channel capability

Battery Low Indicator

Adjustable Audio Gain (+3dBu to -30dBu)

Frequency Range: 170-220MHz

Power Output: typ 20mW, 2mW ERP Deregulated Channels

Audio Frequency Response: 70Hz-18kHz

Audio Input: Lemo FGG304

Dimensions: 60 x 25 x 95mm

Weight: 100g

Fully meets with requirements of ETS300-422/455

 

S3.2MTX TRANSMITTER
Frequency Range: 170-220MHz

Power Output: typ 20mW, 2mW ERP Deregulated Channels

Nominal Deviation: 22kHz

Audio Frequency Response: 70Hz-18kHz

available with high quality uni-directional dynamic head MU-48C (others available on request)

Easy battery access

Dimensions: 235 x 50 x 30mm

Weight: 200g

Fully meets with requirements of ETS300-422/455

 

S3.2GTX TRANSMITTER
As specification for S3.2LTX except for:

Audio Frequency Response: 40Hz-18kHz

Audio Input: 1/4" Mono Jack




