	S4.5 UHF MICROPHONE SYSTEMS


	

	THE SYSTEM

Based on the award winning S4000, the new Trantec S4.5 UHF system boasts a multi-function receiver, 4 frequency switchable channels and the latest PLL tuning technology, making it the ultimate choice when up to 4 frequencies are required. It can be used license free in the UK on channel 70.

The S4.5 systems is avaialble in lapel and headworn microphone versions, two handheld versions (dynamic and condenser) and a dedicated guitar system.

The user friendly multi-function Switchable Receiver LCD display shows chosen frequency selection, RF level, VU, Mute Level, User Identifaction and Antenna Recognition System, while the Transmitter LCD shows currently selected frequency and bank. 


	THE RANGE

S4.5G: guitar system
S4.5L: beltpack system
S4.5LM: as S4.5L but with TS259 lapel microphone
S4.5LHM: as S4.5L but with TS912 headband microphone
S4.5WHM: as S4.5L but with TS44 headband microphone
S4.5MC: handheld system with condenser head transmitter
S4.5MD: handheld system with dynamic head transmitter

All S4.5 systems come complete in a carrying case and are supplied with all necessary antenna, power supply and alkaline battery


	OPTIONAL ACCESSORIES

S4000ADU: Antenna Distribution Unit (up to 4 receivers)
S4000PDU: Power Distribution Unit (up to 4 receivers)
S4000RK: Rack Mounting Kit for two receivers
S5000RD: Remote Dipole Antenna 



	
	TECHNICAL SPECIFICATIONS
 

S4.5RX RECEIVER
RF Frequency Range: Standard Channel 70 Spot Frequencies; 863.025, 863.725, 864.300, 864.500MHz (Others in channels 62-64 or 67-69 available on request)

4 Channel Capability

Audio Frequency Response: 30Hz-18kHz (-3dB)

Dynamic Range: >110dBA

Audio Output Levels: 0dB Unbalanced, -20dB XLR Balanced

Display: Multi-functional LCD with VU/RF levels, Channel info, Mute info, User Name programmability

DC Input: 10.5-18V, 250mA Unregulated. Protected against reverse polarity

Dimensions: 210 x 165 x 30mm

Weight: 900g

 

S4.5LTX TRANSMITTER
10 hour battery life (9v Alkaline Battery)

4 Channel capability

Battery Low Indicator

Adjustable Audio Gain

Power Output: typ 30mW (24MHz -1dB)

Audio Frequency Response: 70Hz-18kHz (-3dB)

Audio Input:Lemo FGG304, 10k Impedance

Dimensions: 60 x 25 x 95mm

Weight: 100g

Fully meets with requirements of ETS300-422/455

 

S4.5MTX TRANSMITTER
4 Channel Capability

Integral LCD Display

User controlled Digital Gain Adjust

Available with high quality uni-directional dynamic head MU-48C or condenser head

Power Output: typ 30mW (24MHz -1dB)

Audio Frequency Response: 70Hz-18kHz (-3dB)

Dimensions: 235 x 50 x 30mm

Weight: 200g

Fully meets with requirements of ETS300-422/455




