
Steps to replace DOM in DLA 1200/1400series

– Prior to replacing the DOM, make sure the DLA is powered off.

– Once powered down, remove the power cords.

– After opening up the DLA, please verify that the green LED on the motherboard is off

– After this you can remove the old DOM and place the new DOM inside the DLA in the same manner

Once the DOM has been physically replaced, close the top lid, reconnect all the power cords and power the unit back on.

During boot up press F11 after the BOSCH Boot logo to enter the menu where you are able to select a boot device; Select the DOM/USB and then wait for the unit to reach the system maintenance menu. 
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You will  now come to the system maintenance menu. Select option 1. initial setup.
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The re-imaging process will now begin. You will see an indication of the remaining time to complete the process.
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Once this process has been completed, please reboot the system again using option 0. During this next reboot the system should act the same way as when it just came out-of-the-box. Simply let the boot process take its course and eventually you will see the following screen
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You can now log in using the following credentials

User Name : Administrator

Password: WSS4Bosch

example for 1200 Series





example for 1400 Series 1U
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