
FIRMWARE RELEASE NOTES
=====================

This doument presents an overview of the new features, enhancements, bug fixes and visible changes in firmware.
----------------------------------------------------------------------------------------------------------------------------------------------------

Product affected:           SNB-6004/6003, SND-6084/6083, SNV-6084R, SND-6084D, SNO-6084R

Release date:         2015-11-02

Firmware version:           v3.03_150918

Firmware file name:         snb6004_Series_v3.03_150918

----------------------------------------------------------------------------------------------------------------------------------------------------

UPGRADE INSTRUCTIONS
=====================

The firmware can be upgraded through the web viewer.
Please follow the instructions from the user manual of SNB-6004/6003, SND-6084/6083, SNV-6084R, SND-6084D, SNO-6084R, the web page at 'http://www.samsungsecurity.com/'.

 

----------------------------------------------------------------------------------------------------------------------------------------------------

Release Information
=====================


New Features
=====================

3.00	 * Apply WR4.0 Platform
		- Support IE 11 for webviewer
		- Support Open Platform 2.0
		- Support interworking between NAS and SD memory card
		- Support backup of log file
		- Support Manual Recording
		- Improve processing speed with CGI command
		- Improve the ONVIF eventservice
		- Improve structure of the webviewer tree menu
		- Improve performance of UTC Playback
	Support P-iris on Dome type camera
	Support area setting on Simple Focus
2.00   	Add RS485 protocol
	Support Smart Codec
        	Support Open Platform
        	Support Image Preset(Direct OSD)
        	Support external zoom and focus control by ONVIF
        	Support recording on NAS
        	Support setting up conversion point of Day and Night
        	Support P-iris manufactured by Tamron


Improvements and Changes
=====================

3.03	Improve performance for RS-485 protocol
	Improve operation of Alarm Input
	Improve stability with ONVIF protocol
3.00	 * Apply WR4.0 Platform
		- Support IE 11 for webviewer
		- Support Open Platform 2.0
		- Support interworking between NAS and SD memory card
		- Support backup of log file
		- Support Manual Recording
		- Improve processing speed with CGI command
		- Improve the ONVIF eventservice
		- Improve structure of the webviewer tree menu
		- Improve performance of UTC Playback
	Improve usability of Image Preset
	Improve performace of D/N Filter
	Add 'MD event blocking function' during switching over to Day mode or Night mode
	Improve security setting
2.23	Improve performance of saving and playing data on SD memory card
2.22	Improve compatibility with SRN-4000 by SUNAPI 2.0
2.21	Improve security setting
2.10    Improve performance of IRIS
2.00    Improve performance of VA and Face detection
        Add protocol for improvement of sequence image quality
        Change default mode for monitoring  in web viewer to Fit mode 
        Add ATC available protocol on RTP connecting
        Improve performance of DIS for optimizing all ability range of zoom ratio


