1998 price list - page 2

NET LOGICS FOR ACCESS CONTROL AND PRESENCE CONTROL

BCA NET/H Serial logic board with multi I/O remotizable on two-wire line (S-ART or S-ARR modules) ideal for control of hotel rooms or as alarm concentrator: complete control of 4 access points, 700 codes and 1.000 events as basis, with possible expansion x2 (requires EXP BCA/2) ___________________________________

PLW NET Advanced technology serial logic board (without container) for high security, high flexibility access control, complete control of 6 access points, 850 codes and 500 events as basis, with possible expansion x2, x4, x8 (requires EXP NET/2, /4, /8) _________________________________________________________

____ 1.523.000

____ 1.586.000

CONCENTRATOR LOGIC BOARDS

Logic boards for control of multiple accesses for interfacing with non-dedicated PC for programming and data upload. Management of from 500 to 30,000 different codes. A basic software package for programming stand-alone use mode is supplied. Capability for management in RS485 network of 127 different logic boards and terminals. Direct connection to modem for remote interrogation (requires ^SFW

M~). Compatible with PLW peripherals. Power supply at 24 Vdc.

UCA NET Terminal with two-way wipe-over magnetic badge reader, control of 700 codes and 1.000 events as basis, with possible expansion x2 (requires EXP BCA/2) __________________________________________

UCA PROX Terminal with proximity microchip reader (ARIS), control of 700 codes and 1.000 events as basis, with possible expansion x2 (requires EXP BCA/2) ______________________________________________

ULB NET Terminal with two-way wipe-over magnetic badge reader, complete control of 6 access points, 880 codes and 500 events as basis, with possible expansion x2, x4, x8 (requires EXP NET/2, /4, /8) ___________

ULB PROX Terminal with proximity microchip reader (ARIS), complete control of 6 access points, 880 codes and 500 events as basis, with possible expansion x2, x4, x8 (requires EXP NET/2, /4, /8) __________________

____ 2.003.000

____ 2.950.000

____ 3.108.000

____ 4.260.000

TERMINALS

Logic units with keyboard and backlit displayfor presence control for interfacing with non-dedicated PC for programming and data upload.

Management of from 500 to 30,000 different codes. A basic software package for programming stand-alone use mode is supplied.

Capability for management in RS485 network of 127 different logic boards and terminals. Direct connection to modem for remote interrogation (requires ^SFW M~). Compatible with PLW peripherals. ULB NET and ULB PROX terminals may be used to allow access control for

6 complete access points. Power supply at 24 Vdc.

EXP BCA/2 RAM memory expansion of 32 Kb x 2 for BCA NET/H, UCA NET and UCA PROX_________________

EXP NET/2 RAM memory expansion of 32 Kb x 2 for PLW NET, ULB NET and ULB PROX ___________________

EXP NET/4 RAM memory expansion of 32 Kb x 4 for PLW NET, ULB NET and ULB PROX ___________________

EXP NET/8 RAM memory expansion of 32 Kb x 8 for PLW NET, ULB NET and ULB PROX ___________________

COM 485 Screened, twisted data cable specifically for RS485 communications (per metre) __________________

COM 485/G Screened, twisted data cable specifically for RS485 communications, especially for applications in disturbed environments (per metre) ________________________________________________________

CNT A1 Plastic container for PLW NET - dimensions: 125 x 230 x 210 mm______________________________

ML 485 RS485 interface module for connection of several PLW NET, ULB NET and ULB PROX logic units together, with other terminals and concentrators and/or to PLC located more than 15 metres away _____

CVT 485 RS232 - RS485 conversion interface for installation close to PC for connection of logic boards and/or terminals (with ML 485 module on board when necessary) - power supply 220 VAC________________

CVT 485/M Multiple RS232 (1 IN) - RS485 (4 OUT) conversion interface __________________________________

S-ART Serial module on two-wire line 2 IN + 2 logic OUT for BCA NET/H logics ________________________

S-ARR Serial module on two-wire line 2 logic IN + 2 OUT for BCA NET/H logics ________________________

_____ 105.000

_____ 105.000

_____ 263.000

_____ 525.000

_______ 4.000

______ 13.000

_____ 110.000

_____ 356.000

_____ 434.000

____ 1.302.000

______ 70.000

______ 90.000

NET LINE ACCESSORIES

Accessories for NET terminals and logic boards. RAM memory expansions for increasing the potential of systems x2, x4, x8. Interfaces for

RS232 - RS485 standards for connections in network and with PC. Specific screened RS485 data cables for critical applications in disturbed environments.

SFW CA1 Advanced technology access control for systems from 1 to 3 concentrators or terminals ____________

SFW CA3 Advanced technology access control for systems from 4 to 127 concentrators or terminals __________

SFW M Additional software module for modem control, for direct connection of a logic board, a terminal or a network of logic boards and/or terminals to a modem for download of data from PC by switched telephone line ___

SFW F Additional time-band software module for SFW CA1 and CA3 _________________________________

SFW S Additional badge expiry date software module for SFW CA1 andCA3 ___________________________

SFW P Additional P.I.N. and anti-coercion software module for SFW CA1 and CA3_______________________

SFW B Additional anti pass-back software module for SFW CA1 and CA3 _____________________________

SFW CP Additional presence control software module for SFW CA1 and CA3 ____________________________

_____ 840.000

____ 1.995.000

_____ 900.000

_____ 158.000

_____ 158.000

_____ 263.000

_____ 525.000

_____ 945.000

SOFTWARE

Further additional modules can be optionally used for functional implementations. The SFW M module requires an external modem,

14.400 bps, V.32 bis, autoanswer or superior, connected to the Access Control and/or Presence Management system.

1998 price list - page 3

PLW DECODERS FOR ACCESS CONTROL

PLW 382 PLW serial keyboard in polycarbonate with 3 code decoder with 3 built-in relays for access control; possibility of connection to other PLW peripherals, also ideal for use outdoors - projecting installation ______

ACCESSORIES:

CNT 3P Outdoor rain shelter in black anodized aluminium for PLW 382 ________________________________

_____ 220.000

______ 24.000 ordering.

PLW 232 Conversion interface from PLW line to RS232 and Centronics standards (specify number of printer columns if different from 80) - requires PLW serial keyboard or Personal Computer for date and time programming_____ 466.000

PLW PRN 2 24 column event recorder impact printer - Centronics parallel output ________________________________ 1.213.000

PLW 380/1 Decoder with 30 numerical codes and 1 relay in plastic container ______________________________

PLW 380/3 Decoder with 3 numerical codes and 3 relays in plastic container (requires programming keyboard) ___

PLW 380/128 Decoder with 126 numerical codes and 1 relay in plastic container _____________________________

PLW 380/500 Decoder with 500 numerical codes and 1 relay in plastic container _____________________________

PLW 380/MR1 Decoder with 126 numerical codes and 4 on-board relays which can be increased up to 64 using PLW

380/RA modules - codes associated to 1 or more relays (requires programming keyboard) - housed on

DIN rail ____________________________________________________________________________

PLW 380/MR2 Decoder with 126 numerical codes and 4 on-board relays which can be increased up to 16 using PLW

380/RA modules - peripherals associated to 1 relay - housed on DIN rail ________________________

PLW 380/RA 4 relay module for PLW 380/MR - housed on DIN rail ________________________________________

PLW DT4 Telephonic decoder with 4 numerical codes and 4 on-board relays (requires programming keyboard) - housed on DIN rail ___________________________________________________________________

PLW SERIAL DECODERS

Access control units which control PLW peripherals for activation of on-board relays by means of numerical codes, also sent as DTMF pulses from telephone line. Each decoder controls up to 16 PLW peripherals in a network; these peripherals may be keyboards, magnetic badge readers and proximity microchips. The various models of decoder manage from 3 to 500 different codes and from 1 to 64 on-board relays.

PLW^COMPACTS~: KEYBOARD + DECODER

3 relay decoder with built-in keyboard for programming, with possibility of connection to PLW peripherals for data acquisition by means of numerical codes and/or personal magnetic badges for access control, usable as stand-alone systems, for subdivision of burglar alarm systems, etc.

INTERFACES

Interface for converting output signals from the PLW decoders into common standards for passage reports on printer and/or on-line PC, also usable for programming of codes on the decoder from PC. The PLW 232 conversion interface, which allows connection of a decoder to PC and/or to on-line printer, is supplied with output for 80 column printers; state any requests for modifications to this standard when

PRINTERS

24 column impact printer, power supply 220 VAC. For connection to access control systems with PLW decoder, requires PLW 232 conversion interface. Ideal for installation in security cabinets. The PLW PRN 3 version can also be ordered with 24 Vdc. power supply

(state when ordering).

_____ 113.000

_____ 163.000

_____ 182.000

_____ 293.000

_____ 396.000

_____ 396.000

_____ 176.000

_____ 290.000

1998 price list - page 4

PLW PERIPHERALS FOR ACCESS CONTROL

PLW 380/TP 12 key serial keyboard for outdoor use in scratch-proof polycarbonate - projecting installation ________

PLW 380/TAL 12 key serial keyboard in white anodized aluminium - projecting installation ______________________

PLW 380/OT 12 key vandal-proof serial keyboard for outdoor use in treated brass polycarbonate - inset installation _

PLW 385 10 key serial keyboard for indoor use on Ticino Living_® mechanics - inset installation _______________

PLW 386/TIN 13 key serial keyboard for outdoor use in TerraneoTersystem 2000_® mechanics - inset installation ____

PLW 386/TSP 13 key serial keyboard for outdoor use in Terraneo Tersystem 2000_® mechanics - projecting installation

PLW 387 12 key serial keyboard for indoor use on Vimar idea_® mechanics - inset installation ________________

PLW 388 Vandal-proof serial keyboard for outdoor use in painted steel with security lock with key and cylinder; 12 keys, nighttime illumination - Projecting installation __________________________________________

ACCESSORIES:

GN 380/TP Protective rubber sheath for PLW 380/TP for use outdoors____________________________________

_____ 110.000

_____ 150.000

_____ 915.000

_____ 110.000

_____ 334.000

_____ 390.000

_____ 110.000

_____ 289.000

_______ 6.000

PLW 760/ST PLW wipe-over serial reader for indoor or outdoor use in white anodized aluminium, ISO 2 track - projecting installation _______________________________________________________________________

PLW 760/IN PLW insertion serial reader for outdoor use in white anodized aluminium, ISO 2 track - inset installation - waterproofed as standard______________________________________________________________

PLW 765 PLW serial reader for indoor use on Ticino Living_® mechanics, ISO 2 track - inset installation_________

PLW 767 PLW serial reader for indoor use on Vimar Idea_® mechanics, ISO 2 track - inset installation __________

ACCESSORIES:

CNT 7A White anodized aluminium outdoor rain shelter for PLW 760/ST _______________________________

CNT 7B Anodized aluminium mounting box for PLW 760/IN __________________________________________

CNT 7C Black anodized aluminium outdoor rain shelter for PLW 760/IN (requires CNT 7B for installation on wall or door/window frame) __________________________________________________________________

CNT 7D Free-standing supporting column for outdoor use in galvanized, painted iron (RAL 2004) for PLW 760/IN badge insertion reader ________________________________________________________________

CNT 7M Galvanized steel box for insetting in wall for PLW 760/IN badge insertion reader___________________

IMP 760 Waterproofing process for PLW readers except for PLW 760/IN for outdoor use (surcharge added to list price of individual reader) ______________________________________________________________

TK3 Replacement of ISO 2 track reader head for badges coded with ISO 3 track (surcharge added to list price of individual reader) __________________________________________________________________

PRS Personalization of reading head to use badges with significant fields other than the first 8 (Plexa standard), to be added for each order_________________________________________________________

_____ 560.000

_____ 685.000

_____ 400.000

_____ 400.000

______ 36.000

______ 70.000

______ 36.000

_____ 647.000

______ 28.000

_____ 105.000

______ 90.000

_____ 105.000

SERIAL KEYBOARDS

PLW peripherals for data acquisition by means of personal numerical codes for access control, for connection to NET logic boards

(addressing required on order) or PLW decoder. The Ticino Living_® and Vimar idea_® versions are supplied with polycarbonate for horizontal installation; specify any modifications required to this standard when ordering.

SERIAL READERS FOR ISO 2 TRACK MAGNETIC BADGES

PLW peripherals for access control data acquisition by means of personal magnetic badges coded in Plexa standard (ISO 2 track, first 8 characters) for connection to PLW decoders or logic boards. Possibility of replacing ISO 2 track head with ISO 3 track version (requires

TK3) and/or of reading codes in positions other than the Plexa standard (first 8 characters - requires PRS). When ordering, specify the need to use the customer´s badges to allow the necessary personalization.

PLW^COMPACTS~: KEYBOARD + READER

PLW peripherals for data acquisition by means of numerical codes and/or personal magnetic badges for access control, for connection to

PLW decoders or logic boards. Possibility of replacing ISO 2 track head with ISO 3 track version (requires TK3) and/or of reading codes in positions other than the Plexa standard (first 8 characters - requires ^PRS~). When ordering, specify the need to use the customer´s badges and/or the need to use the keyboard always combined with the reader (^non automatic ENTER~) to allow the necessary personalization.

PLW 1140/LT PLW serial unit, 12 key keyboard + wipe-over magnetic badge reader, ISO 2 track - projecting installation

ACCESSORIES:

TK3 Replacement of ISO 2 track reader head for badges coded with ISO 3 track (surcharge added to list price of individual reader) __________________________________________________________________

PRS Personalization of reading head to use badges with significant fields other than the first 8 (Plexa standard), to be added for each order_________________________________________________________

_____ 668.000

______ 90.000

_____ 105.000

1998 price list - page 5

ARIS PROXIMITY IDENTIFICATION SYSTEM

PAR PLW Control module in plastic container 135 x 85 x 32 mm for use with PAR A0/A, PAR A0/L, PAR A0/V, PAR

A1 and PAR A2 antennas ______________________________________________________________

PAR PLW/A Control module in plastic container 166 x 118 x 75 mm for use with PAR A3, PAR A4, PAR A5, PAR A6,

PAR A7 and PARAV antennas__________________________________________________________ ____ 1.447.000

____ 1.447.000

PAR A0/A Proximity reading antenna for indoor use in 1 Ave_® module - dimensions 25 x 45 x 40 mm, range up to 20 cm with PAR TC _____________________________________________________________________

PAR A0/L Proximity reading antenna for indoor use in 1 Ticino Living_® module - dimensions 25 x 45 x 40 mm, range up to 20 cm with PARTC ______________________________________________________________

PAR A0/V Proximity reading antenna for indoor use in 1 Vimar idea_® module - dimensions 25 x 45 x 40 mm, range up to 20 cm with PARTC _________________________________________________________________

PAR A1 Vandal-proof outdoor proximity reading antenna in module for installation in masonry - dimensions 40 x

20 x 2 mm - range up to 20 cm with PARTC - inset installation ________________________________

PAR A2 Outdoor proximity reading antenna in polycarbonate container - dimensions 75 x 105 x 30 mm - range up to 40 cm with PARTC - projecting installation ______________________________________________

PAR A3 Panel type outdoor proximity reading antenna - dimensions 270 x 720 x 10 mm - range up to 70 cm with

PAR TC - projecting or inset installation ___________________________________________________

PAR A4 Panel type outdoor proximity reading antenna - dimensions 520 x 940 x 10 mm - range up to 100 cm with

PAR TC - projecting or inset installation ___________________________________________________

PAR A5 Indoor proximity reading antenna in structureless version for pedestrian use for hands-free access control

- dimensions 800 x 2000 cm - range: total coverage of passage through access point with PARTC - shape and size can be personalized on request - inset installation ___________________________________

PAR AV Completely airtight outdoor proximity reading antenna for use with vehicles, for installation sunk into the ground - dimensions 1000 x 2000 mm approx. - range up to 170 cm with PARTV - shape and size can be personalized on request - inset installation ________________________________________________

PAR A7 Outdoor proximity reading antenna in painted PVC for use with vehicles - installation on 60 mm road-sign post - dimensions 590 x 1150 x 100 mm - range up to 200 cm with PARTD ______________________

_____ 168.000

_____ 168.000

_____ 168.000

_____ 200.000

_____ 320.000

_____ 630.000

_____ 840.000

_____ 378.000

_____ 630.000

____ 1.870.000

PAR TC Pedestrian proximity transponder, ISO standard badge format - dimensions 86 x 54 mm.____________

PAR TG Capsule format proximity transponder in impact-resistant sterilizable glass - dimensions: dia. 3.8 x 23 mm.

PAR TK Key-ring or watch format pedestrian proximity transponder - dimensions: 42 x 33 x 7 mm. ___________

PAR TS Disc format pedestrian proximity transponder - dimensions: dia. 30 x 6.5 mm._____________________

PAR TD Disc format vehicle windscreen proximity transponder - dimensions: dia. 86 x 5 mm. _______________

PAR TV Cylindrical format vehicle proximitytransponder in impact-resistant material - dimensions: 130 x 30 x 18 mm.

______ 29.000

______ 39.000

______ 44.000

______ 39.000

______ 50.000

_____ 140.000

UCPRX1 Proximity reading antenna with built-in control module for indoor use - dimensions: 130 x 80 x 27 mm - range up to 50 cm with PARTC - completely projecting installation _________________________________ 1.905.000

CONTROL MODULES

Control modules for ARIS line proximity antennas. Provide power supply to the connected antennas (one antenna every PARPLW or PAR

PLW/A control module) and decoding of the codes received from the transponders, which are sent to the decoders or logic boards with

PLW communications protocol. Power supply from 20 to 38 Vdc.

ANTENNAS

Controlled by a PAR PLW module, they receive the transponder codes read at a distance for subsequent decoding by PLW logic boards or decoders. They permit extremely user-friendly access control, with vandal-proof or hands-free characteristics if required, with the guarantee of high security and durability thanks to the absence of contact with the transponders.

TAG TRANSPONDERS

Literally ^responders~, the heart and brain of the ARIS systems, they contain a silicon permanent memory with a 64 bit structure which allows generation of over 5,000,000,000 unique code combinations which cannot be duplicated. The absence of batteries guarantees less pollution than with other similar systems, as well as virtually unlimited lifetime.

ARIS PROXIMITY^COMPACTS~: ANTENNA + CONTROL MODULE

Proximity reading unit complete with control module, and communications interface for connection to PLW decoders or logic boards.

Further simplifies the installation of proximity access control. Power supply 20 or 38 Vdc.

1998 price list - page 6

PHYSICAL ACCESS CONTROL SYSTEMS

GATES

Anti-panic one/two-way motor-operated gates and one-way push-open gates in painted steel and polished AISI 304 stainless steel. State the width of the access passage to be covered when ordering.

PASSATOR One/two-way three-bar turnstile in painted steel (uprights and top) and polished AISI 304 stainless steel

(arms and lower tie-rod) - power supply 24 Vdc. ____________________________________________

PASSATOR 2 One/two-way three-bar turnstile in painted steel (uprights) and polished AISI 304 stainless steel (top, arms and lower tie-rod) - power supply 24 Vdc. _____________________________________________

PASSATOR 3 One/two-way three-bar turnstile in polished AISI 304 stainless steel - power supply 24 Vdc. _________

ACCESSORIES:

PASS 1 Aluminium platform to make the turnstile stable even without fixing to the ground __________________

PASS 2 Barrier in polished AISI 304 stainless steel for channelling traffic through the access passage ________

PASS 3 Table-top power supply unit with mimic display panel for complete management of turnstile__________

PASS 4 Impartial control system with random cut-out and local and remote signalling _____________________

PASS 5 Anti-panic system for manual release of each single turnstile arm, allowing the arm to fall ___________

PASS 6 Two-way LED traffic light with 3 colour (red, green and amber) passage indicator arrows ____________

PASS 7 Support in polished AISI 304 stainless steel for installation of ULB NET or ULB PROX terminal on

PASSATOR turnstile __________________________________________________________________

PASS 8 Photocell for inset installation without reflector, for use on PASSATOR turnstiles __________________

PASS PLW One-way magnetic badge reader in painted aluminium with PLW output for connection to NET series logic boards_____________________________________________________________________________

PASSTTL Two-way magnetic badge reader in painted aluminium with TTL output for connection to NET series logic boards_____________________________________________________________________________

PASS ANT Complete anti climb-over system comprising 3 photocells diam.18 mm with adjustable range connected to a sequential logic control board with output for connection to remote alarm_____________________

____ 6.097.000

____ 6.524.000

____ 7.203.000

_____ 861.000

_____ 420.000

_____ 987.000

_____ 998.000

_____ 700.000

_____ 260.000

_____ 560.000

_____ 350.000

_____ 560.000

_____ 500.000

____ 2.100.000

OK PASS One/two-way motor-operated gate in painted steel (upright) and polished AISI 304 stainless steel (gate) - to cover access passages from 60 to 120 cm as ordered - power supply 24 Vdc. __________________

OK PASS 2 One/two-way motor-operated gate in polished AISI 304 stainless steel - to cover access passages from

60 to 120 cm as ordered - power supply 24 Vdc. ____________________________________________

PASS EASY One-way push-open gate for entries or exits in polished AISI 304 stainless steel - to cover access passages from 60 to 120 cm as ordered _____________________________________________________

ACCESSORIES FOR OK PASS:

PASS 2 Barrier in polished AISI 304 stainless steel for channelling traffic through the access passage ________

PASS 3 Table-top power supply unit with mimic display panel for complete management of OK PASS gate ____

PASS 4 Impartial control system with random cut-out and local and remote signalling _____________________

____ 5.250.000

____ 6.160.000

____ 1.463.000

_____ 420.000

_____ 987.000

_____ 998.000

TURNSTILES

Anti-panic one/two-way three-bar turnstiles in painted steel, ideal for indoor or outdoor use for complete access control. Hydraulic damper.

Anti-panic system for automatic unlocking in case of power supply failure. Output for two-way passage counter. Also available in version with anti climb-over system with sequential visual control by means of 3 photocells or with anti-panic release system allowing the individual arms to fall. State the width of the access passage to be covered when ordering.

MONITORED FREE ACCESS POINTS

One/two-way free access points with passage monitoring by means of 3 photocells diam. 18 mm. adjustable range without reflector, with only one barrier and photocells, in polished AISI 3104 steel (PAS-SI) or comprising aluminium platform and two polished AISI 304 steel barriers. Outputs for two-way passage counter. State the width of the access passage to be covered when ordering. Power supply 24 Vdc.

PAS-SI Control system with single barrier for one- or two-way access points, using 3 photocells - dimensions: 920

× 900 mm. _________________________________________________________________________

PAS-SI 2 Control system with double barrier and platform for one- or two-way access points, using 3 photocells - dimensions: 720 × 920 × 900 mm. - cover access passages: 620 mm. __________________________

ACCESSORIES:

PASS 1 Aluminium platform to make the barrier stable even without fixing to the ground ___________________

PASS 2 Barrier in polished AISI 304 stainless steel for channelling traffic through the access passage ________

PASS 3 Table-top power supply unit with mimic display panel for complete management of barrier ___________

PASS 4 Impartial control system with random cut-out and local and remote signalling _____________________

____ 2.290.000

____ 3.535.000

_____ 861.000

_____ 420.000

_____ 987.000

_____ 998.000

1998 price list - page 7

PLE,PLT AND PLX STAND-ALONE ACCESS CONTROL SYSTEMS

ICL51 PROGRAMMABLE LOGIC BOARDS

PLE 385 Indoor digital key on Ticino Living_® mechanics, 10 keys, 5 codes and 2 relays_____________________

PLE 386/IN Outdoor digital key on Terraneo Tersystem 2000_® mechanics, 13 keys, 5 codes and 2 relays - led lighting

- inset installation ____________________________________________________________________

PLE 386/SP Outdoor digital key on Terraneo Tersystem 2000_® mechanics, 13 keys, 5 codes and 2 relays - led lighting

- projecting installation ________________________________________________________________

PLE 387 Indoor digital key on Vimar idea_® mechanics, 12 keys, 5 codes and 2 relays ______________________

PLE 388 Vandal-proof outdoor serial keyboard in painted steel with security lock with key and cylinder, 12 keys and

5 codes - projecting installation _________________________________________________________

ACCESSORIES:

PLE PWR Power supply interface module for connecting 2 to 16 PLE line elements together _________________

_____ 198.000

_____ 386.000

_____ 486.000

_____ 198.000

_____ 364.000

______ 24.500

PLT 760/ST Wipe-over indoor reader with head emulation (TTL) output in white anodized aluminium, ISO 2 track - projecting installation _________________________________________________________________

PLT 380/1 TTL decoder with 30 codes and 1 relay for connection to 1 PLT 760/ST _________________________

PLT 380/128 TTL decoder with 126 codes and 1 relay for connection to 1 PLT 760/ST ________________________

PLT KIT Aluminium wipe-over TTL reader + TTL decoder with 30 codes and 1 relay_______________________

ACCESSORIES:

TK3 Replacement of ISO 2 track reader head for badges coded with ISO 3 track (surcharge added to list price of individual reader) __________________________________________________________________

PRS Personalization of reading head to use badges with significant fields other than the first 8 (Plexa standard), to be added for each order_________________________________________________________

_____ 205.000

_____ 142.000

_____ 232.000

_____ 315.000

______ 90.000

_____ 105.000

PAR PLX Indoor proximity reader with 475 code decoder and 1 built-in relay _____________________________

PAR XA ISO standard magnetic badge format proximity microchip with codifiable magnetic strip _____________

PAR XB Key-ring format proximity microchip (dimensions 30 x 30 x 5 mm) ______________________________

PAR XC ISO standard magnetic badge proximity microchip __________________________________________

____ 1.428.000

______ 24.000

______ 24.000

______ 22.000

ML 14A Master logic board with 8 opto-insulated two-way inputs (without polarity) and 6 relay outputs ________

ML 36A Master logic board with 20 opto-insulated two-way inputs (without polarity) and 16 relay outputs ______

ICL 51 Development software for programming of ML 14A and ML36A logics, additional modules and accessories _______________________________________________________________________________

PRN1 Standard printer interface slave module for master logics _____________________________________

PTD2 Terminal panel slave module with 16 key keyboard and 32 character display for master logics ________

EXP16A Slave expansion module with 8 opto-insulated two-way inputs (without polarity) and 8 relay outputs ___

EXP36A Slave expansion module with 32 open collector outputs for master logics ________________________

PRG1 RS232/RS485 standard serial interface slave module for master logics with galvanic insulation in plastic container, complete with wires and connectors _____________________________________________

PRG2 RS232/RS485 standard serial interface slave module for master logics __________________________

MLW Clock and calendar slave module for master logics __________________________________________

_____ 564.000

_____ 864.000

_____ 420.000

_____ 342.000

_____ 574.000

_____ 490.000

_____ 900.000

_____ 734.000

_____ 356.000

______ 64.000

DIGITAL KEYS

New concept digital keys and keyboards (with on-board relays) for small access control and/or burglar alarm control systems. Completely replace the Plexa PLX digital key line. Improved compared to the previous version, they feature an increase to 5 numerical codes in memory with ^Night Codes~for temporary disabling of the keyboard and the possibility of network connection of up to 16 elements of the

PLE line (PLE PWR module required for each net). The Ticino Living_® and Vimar idea_® versions are supplied with polycarbonate unit for horizontal installation; state any modifications to this standard required when ordering. Power supply from 12 to 24 Vdc. without polarity.

LOW COST PROXIMITY CHIP READERS

Proximity microchip readers with built-in encoders for stand-alone indoor access controls. 475 personal codes managed by means of ISO standard format badges with or without magnetic strip or key-rings: programming for auto-learning. Maximum range of 15 cm.

Open frame multi I/O logic boards, programmed or programmable by means of software, for control in stand-alone mode or with PC connection of counters, car-parks, interlocks, timing systems, systems with inputs and outputs in general, etc. Housed on DIN rail.

LOW COST MAGNETIC BADGE READERS

ISO standard magnetic badge readers and decoders for stand-alone indoor access control. 5-wire TTL communications between reader and decoders supplied individually or in kits. Connection of just one reader per decoder over a maximum distance of 1 metre. Possibility of replacing ISO 2 track head with ISO 3 track version (requires ^TK3~) and/or of reading codes in positions other than the Plexa standard

(first 8 characters - requires ^PRS~). When ordering, specify the need to use the customer´s badges to allow the necessary personalization.

1998 price list - page 8

PLX STAND-ALONE MAGNETIC READERS

PLX MAGNETIC BADGE CODERS

PLX 725 Indoor insertion type badge-holder pocket on Ticino Living_® mechanics__________________________

PLX 727 Indoor insertion type badge-holder pocket on Ticino Living_® mechanics__________________________

PLX 720/ST Wipe-over magnetic card identifier in track 2 and/or 3 - projecting installation _____________________

PLX 720/IN Wipe-over magnetic card identifier in track 2 and/or 3 - inset installation _________________________

PLX 730/ST Outdoor wipe-over reader with head emulation (TTL) output in white anodized aluminium ISO 2 track - projecting installation _________________________________________________________________

PLX 730/IN Outdoor wipe-over reader with head emulation (TTL) output in white anodized aluminium ISO 2 track - inset installation _____________________________________________________________________

PLX 735 Indoor insertion reader with head emulation (TTL) output on Ticino Living_® mechanics, ISO 2 track - inset installation__________________________________________________________________________

PLX 737 Indoor insertion reader with head emulation (TTL) output on Vimar idea_® mechanics, ISO 2 track - inset installation__________________________________________________________________________

PLX 780/ST Outdoor wipe-over reader with RS232 output in white anodized aluminium ISO 2 track - projecting installation ______________________________________________________________________________

PLX 780/IN Outdoor wipe-over reader with RS232 output in white anodized aluminium ISO 2 track - inset installation _

CNT 7A White anodized aluminium outdoor rain shelter for wipe-over readers ___________________________

CNT 7B Black anodized aluminium mounting box for outdoor insertion readers __________________________

CNT 7C Black anodized aluminium rain shelter for outdoor insertion readers (requires CNT 7B for mounting on wall or door/window frame) ____________________________________________________________

CNT 7D Free-standing outdoor vehicle column in galvanized, painted iron (RAL 2004) for outdoor insertion readers________________________________________________________________________________

CNT 7M Box for installation in masonry in galvanized steel for outdoor insertion readers ___________________

IMP 720 Waterproofing of wipe-over readers for outdoor use (surcharge added to list price of individual reader) _

TK3 Personalization of reading head for badges coded with ISO 3 track (surcharge added to list price of individual reader) ____________________________________________________________________

PLX 767 Magnetic badge coder, low coercivity (300 Oe) with keyboard and display _______________________

PLX 767/H Magnetic badge coder, high coercivity (4.000 Oe) with keyboard and display _____________________

PLX 787 Magnetic badge coder, low coercivity (300 Oe) without keyboard and display, with software package __

PLX 787/H Magnetic badge coder, high coercivity (4.000 Oe) without keyboard and display, with software packaging

_____ 548.000

_____ 646.000

_____ 267.000

_____ 354.000

_____ 205.000

_____ 205.000

_____ 712.000

_____ 845.000

______ 36.000

______ 70.000

______ 36.000

_____ 647.000

______ 28.000

_____ 105.000

______ 90.000

____ 4.400.000

____ 4.600.000

____ 4.000.000

____ 4.200.000

DIMENSIONAL IDENTIFIERS

Dimensional badge identifiers ideal for use in hotel room control systems. Badge-holder pockets for use indoors on Ticino Living_® and

Vimar idea_® standard mechanics, inset installation.

MA GNETIC CARD IDENTIFIERS

ISO standard magnetic badge identifiers ideal for use in access controls for cash-point areas. Possibility of identification of magnetic cards in track 2 (credit cards) and/or track 3 (bank cash cards) with selection even by final customer during installation.

MA GNETIC BADGE READERS

ISO standard magnetic badge readers with standard interface for connection to access control systems and/or on-line connections to PC.

ISO 2 track head can be replaced with one in ISO 3 track (requires ^TK3~).

ACCESSORIES FOR MAGNETIC BADGE IDENTIFIERS

Complete accessories for ISO standard magnetic badge identifiers. Personalization for replacement of ISO 2 track head with one in ISO

3 track (^TK3~). Containers for installation outdoors, set into walls, underwater, etc.

Motor-operated readers/writers for ISO standard track 2 and 3 magnetic badges for independent, personalized coding management.

Possibility of connection to PC by means of RS232 port, on-board display and keyboard or, as an alternative in PLX 787 versions, coding management software in Windows_® environment, and high coercivity reading head (HI.CO at 4,000 Oe).

______ 79.000

______ 79.000

1998 price list - page 9

PLX SYSTEMS AND SENSORS FOR BANK CONTROL

PLX 500 Extremely high performance interlock console for automatic and manual one/two-way control ________

PLX 501 High performance interlock console for automatic and manual one/two-way control ________________

PLX 502 Medium performance interlock console for manual one/two-way control _________________________

PLX 505 Timed interlock for condominium doorway control ___________________________________________

INTERVOX Two-way communications system complete with indoor station comprising a single unit with microphone, speaker and control electronics; outdoor station comprising rod microphone up to 60 cm long (state when ordering) and speaker ________________________________________________________________

PLX 413/OC Indoor reflection photocell with open-collector output, range from 3 to 7 metres - power supply 12/24 Vdc.

PLX 413/RL Indoor reflection photocell with relay output, range from 3 to 7 metres - power supply 24 Vdc. (12 Vdc. on request) ___________________________________________________________________________

ACCESSORIES

PLX 413/C Flat cable connector (specify inter-connector distance)_______________________________________

PLX 440 Piloting unit - power supply at 24 Vdc. (12 Vdc. on request) ___________________________________

CRT 413 Black anodized aluminium casing (per metre) ______________________________________________

PLX 490 Ultra high efficiency reflective tape (per metre) _____________________________________________

PLX 416 Control electronics without beams with relay output _________________________________________

PLX 416/R Projector + receiver pair for beams at interspace 35 mm or multiples ____________________________

PLX 416/C Double casing in black anodized aluminium (per metre) ______________________________________

PLX 310 Capacitative circuit for single sensitive handle______________________________________________

PLX 330 Capacitative circuit for double sensitive handle _____________________________________________

PLX 420 Dual technology sensor - power supply 24 Vdc. ____________________________________________

PLX 432 Magnetic contact ____________________________________________________________________

PLX 461 Active infrared sensor for indoor use - power supply 12/24 Vdc. ________________________________

____ 2.500.000

____ 1.008.000

_____ 840.000

_____ 231.000

____ 1.418.000

_____ 104.000

_____ 104.000

_______ 6.000

_____ 116.000

_____ 111.000

______ 54.000

_____ 138.000

______ 36.000

_____ 111.000

_____ 158.000

_____ 238.000

_____ 305.000

______ 13.000

_____ 438.000

SENSORS

Dual technology sensors. Magnetic contacts. Circuits for single and double sensitive handles for installation on the moving parts of security doors or capsule access doors; supplied as standard with power supply at 24 Vdc.; specify any modifications required to these standards when ordering.

TELESYNCHRONIZED BARRIER OPTIC BARS

Telesynchronized barrier optic bars for signalling alarms or presence inside banks or public premises in general. When ordering, state beam interspace and barrier length. For indoor installation only.

REFLECTION OPTIC BARRIERS AND PHOTOCELLS

Barrier optic photocells for signalling alarms or presence inside banks or public premises in general. When ordering, state photocell interspace and length of casing in case of complete barrier (requires CRT 413, PLX 413/C and PLX 440). For indoor installation only.

INTERPHONES

Live voice communication system between indoor and outdoor positions separated by bullet-proof security glass, ideal for banks and public and private offices.

CASH-POINT AREA CONTROL KIT

Kit for control of access to and time spent in cash-point areas. Comprises control unit, power supply unit with battery charger, plastic container, wipe-over track 2 and/or 3 magnetic badge identifier (replaceable with a PLX 720/IN insertion identifier as required), two aluminium traffic-lights (indoor with 2 messages with time request button, and outdoor with 4 messages), dual technology sensor and magnetic proximity stop for door closed position.Allowing complete, timed, personalizable management of the cash-point area, including multi-message voice syntheses, remote alarms, etc. (optionals to be stated when ordering).

INTERLOCK CONTROL UNITS

High professional interlock control units and consoles for banking or residential applications. Control kits complete for access door capsule are designed for completion with traffic lights, intercoms, sensitive handles, photocells, etc., depending on specific requirements.

PLX 611 Complete kit for access control and presence management for cash-point areas __________________

PLX 612 Simplified kit for access control and presence management for cash-point areas __________________ ____ 3.800.000

____ 2.580.000

1998 price list - page 10

PLX INDICATORS FOR BANK CONTROL SYSTEMS

PLX EMERGENCY DOOR CONTROL SYSTEMS

PLX 470/2 Aluminium traffic light with 2 messages ^COME IN - WAIT~, in two colours (green and red) __________

PLX 470/4 Aluminium traffic light with 4 messages ^WAIT - FREE - CLOSED - COME IN~, in two colours (green and red) _______________________________________________________________________________

PLX 470/RT Aluminium traffic light with 1 message ^REQUEST TIME~ and time request button in 1 colour (red) ____

PLX 470/F Aluminium traffic light with 2 messages ^COME IN - WAIT~, in two colours (green and red) and illuminated button _____________________________________________________________________________

PLX 475 Traffic light in Ticino Living_® mechanics with message ^OPEN DOOR~ and illuminating button in two colours (green and red) - horizontal installation _______________________________________________

PLX 475/2 Traffic light in Ticino Living_® mechanics with 2 messages ^COME IN - WAIT~, in two colours (green and red)

PLX 475/4 Traffic light in Ticino Living_® mechanics with 4 messages ^WAIT - FREE - CLOSED - COME IN~, in two colours (green and red) _______________________________________________________________

PLX 475/RT Traffic light in Ticino Living_® mechanics with 1 message ^REQUEST TIME~ in one colour (red) and time request button_______________________________________________________________________

ACCESSORIES:

CNT 7A White anodized aluminium outdoor rain shelter for PLX 470 ___________________________________

IMP 470 Waterproofing of PLX 470 traffic lights for outdoor use _______________________________________

PLX 480/F Outdoor intercom unit in anodized aluminium (140 x 40 x 11 mm) - projecting installation ___________

PLX 485 Outdoor intercom unit in Ticino Living_® mechanics - vertical inset installation _____________________

PLX 480 Outdoor intercom unit in anodized aluminium (180 x 40 x 11 mm) complete with traffic light section - projecting installation _________________________________________________________________

ACCESSORIES:

CNT 7A White anodized aluminium outdoor rain shelter for PLX 480 ___________________________________

IMP 480 Waterproofing of PLX 480 intercom for outdoor use _________________________________________

PLX 481 Intercom interface for Terraneo_® indoor unit ________________________________________________

PLX 481/P Intercom interface in plastic container for two-way communications system with console indoor unit ___

PLX C2/A Voice synthesis unit with 2 pre-recorded messages (requires DGT C2) for total of 8 seconds without container ___________________________________________________________________________

PLX C2/AR Voice synthesis unit with 2 messages recordable by user for total of 8 seconds without container _____

PLX C2/B Voice synthesis unit with 2 pre-recorded messages (requires DGT C2) for total of 32 seconds without container ___________________________________________________________________________

PLX C2/BR Voice synthesis unit with 2 messages recordable by user for total of 32 seconds without container ____

PLX C12 Voice synthesis unit with 1 message recordable by user lasting 12 seconds, in plastic container ______

ACCESSORIES:

DGT C2 Digitization of messages from cassette for recording on PLX C2/AR and/BR (depending) ___________

CNT C2 Plastic container for PLX C2 (100 x 100 x 55 mm) __________________________________________

_____ 287.000

_____ 412.000

_____ 357.000

_____ 256.000

_____ 240.000

_____ 223.000

_____ 412.000

_____ 268.000

______ 36.000

_____ 105.000

_____ 200.000

_____ 197.000

_____ 343.000

______ 36.000

_____ 105.000

_____ 208.000

_____ 290.000

_____ 260.000

_____ 340.000

_____ 420.000

_____ 500.000

_____ 300.000

______ 13.000

______ 32.000

TRAFFIC LIGHTS

Optic indicators for banking, civil and industrial systems. Supplied as standard with power supply at 24 Vdc., negative switching, white anodized aluminium; specify any modifications required to these standards when ordering. The versions in Ticino Living_® mechanics are all for vertical inset installation except for PLX 475.

INTERCOMS,TRAFFIC LIGHTS + INTERCOMS

Optic indicators and intercoms for banking, civil and industrial systems. Supplied as standard with power supply at 24 Vdc., negative switching, white anodized aluminium; specify any modifications required to these standards when ordering.

VOICE SYNTHESIS UNITS

Voice synthesis units with one or two messages for interlock systems of banks and public systems in general. All two message voice synthesis units, supplied without container, are available in version which can be recorded by the final user by means of built-in microphone or in the pre-recorded version (requires DGT C2).

Control unit and management console for one emergency door provided with complete acoustic and visual alarm diagnostic. Allows unlocking timed control (from 0" up to 40") and acousting alarm signalling door opening.

CPE 10 Control unit and management console for one emergency door _____________________________________ 696.000

1998 price list - page 11

ACCESSORIES

STANDARD, NON STANDARD, BLANK OR PERSONALIZED BADGES

AL 15 Power supply unit for decoderless PLW line, direct power supply to PLW serial keypads or readers____

AL 4024 24 Vdc, 1,8A power supply unit - without containter _________________________________________

AL 6024 24 Vdc, 2,5A power supply unit - without containter _________________________________________

AL 24024 24 Vdc, 10A power supply unit - without containter __________________________________________

AL 54VA 24 Vdc, 2,5A power supply unit with battery charger - without container _________________________

AL 590 24 Vdc, 8A switching power supply unit with battery charger - without container ___________________

PLX SRN Indoor 110dB siren, provided with bracket - power supply 12 Vdc - dimensions 43x40x58 mm. _______

ACCESSORIES

BATT 12/2 12 Vdc, 2Ah buffer battery _____________________________________________________________

BATT 12/6 12 Vdc, 6Ah buffer battery _____________________________________________________________

CNT A1 Plastic container for AL24024, AL 590 - dimensions 125x230x310 mm. _________________________

CNT A2 Plastic container for AL 4024, AL 6024, AL 54VA - dimensions: 100x195x210 mm. ________________

PLX 580 Electric piston lock - power supply 24 Vdc. ________________________________________________

PLX 580/A Electric piston lock in anti-panic version - power supply 24 Vdc. ________________________________

PLX 581 Electric stop, lightweight version - power supply 24 Vdc. ______________________________________

PLX 581/B Electric stop, security version - power supply 24 Vdc. ________________________________________

ELM 180 Miniature electromagnet for surface installation, retention of over 180 kg. ________________________

ELM 300 Electromagnet for inset installation, retention of over 300 kg. __________________________________

ELM 500/S Single electromagnet with LED, retention of over 500 kg. _____________________________________

ELM 500/D Single electromagnet with LED, retention of over 500 kg. _____________________________________

ACCESSORIES:

ELM V Double L and Z bracket for fixing the counter-plate of the ELM 500/S ___________________________

ELM L L bracket for fixing the counter-plate of the ELM 500/S _______________________________________

ELM z Z bracket for fixing the counter-plate of the ELM 500/S _______________________________________

_____ 105.000

_____ 214.000

_____ 235.000

_____ 615.000

_____ 426.000

_____ 566.000

______ 45.000

______ 48.000

______ 67.000

_____ 110.000

_____ 100.000

_____ 700.000

_____ 700.000

_____ 520.000

_____ 958.000

_____ 312.000

_____ 347.000

_____ 545.000

____ 1.055.000

_____ 221.000

_____ 170.000

_____ 170.000

ELECTROMAGNETS FOR EMERGENCY DOORS

Electromagnets at 12/24 Vdc.for applications on single or double emergency doors. Extremely high resistance to stresses up to over 500 kg. Power supply from 12 to 24 Vdc.

POWER SUPPLY UNITS, BATTERIES AND SIRENS

Power supply units for all Plexa product lines. Supplied with or without built-in battery charger.

ELECTRIC LOCKS, ELECTRIC STOPS

Accessories for all Plexa product lines. Accessories for all Plexa product lines. Electric piston locks and electric stops for civil and/or banking applications. Power supply 24 Vdc.

PVC magnetic badges, ISO standard 0.76 mm for Plexa readers. Coding with Plexa standard envisages consecutive numbering of 8 characters, guaranteeing uniqueness, with punching in legible form on the badge; all requests for punching and/or coding with numbers to customer specification are considered ^non Plexa standard~. For personalization with thermal sublimation printing, provide outline instructions for production, an original of the colour logotype and/or photographs for printing on the badge. Personalized printing is always on one side of the badge (specify if required on back).

PLW 720/T Blank white badges with magnetic band with low coercivity (300 Oe) (not coded, not punched and not printed).

PLW 760/T Standard white badges with magnetic band with low coercivity (300 Oe) (coded and punched with Plexa standard).

PLW 760/TM Standard badges with magnetic band with low coercivity (300 Oe), with monochrome printing (coded and punched with Plexa standard).

PLW 760/TC Standard badges with magnetic band with low coercivity (300 Oe), with 256-colour printing (coded and punched with Plexa standard).

PLW 760/FT Standard badges with magnetic band with low coercivity (300 Oe), with 256-colour printing with passport photograph, (coded and punched with Plexa standard).

PLW***/H Badges in version with high coercivity magnetic band (HI.CO. at 4000 Oe), coded and punched with Plexa standard

PLW PLW PLW PLW PLW PLW PLW PLW PLW PLW

Quantity

720/T 720/TH 760/T 760/TH 760/TM 760/TMH 760/TC 760/TCH 760/TF 760/TFH

1-50 950 1.045 4.700 5.170 7.400 8.140 10.800 12.000 18.800 21.600

51-100 900 990 3.600 3.960 5.800 6.380 9.800 10.900 17.900 19.700

101-500 800 880 2.900 3.190 5.000 5.500 9.000 10.000 16.400 18.000

501-1000 650 715 2.500 2.750 4.500 4.950 8.100 9.100 to order to order

Customers may also order: - Badges with coding and punching to specification (non Plexa standard) with a surcharge on the list prices of 10%; state the numbering for punching, the numbering of coding and the ISO track (2 and/or 3) to be used.

- Badges in special assortments and quantities to be agreed (separate quotations on request).

1998 price list - page 12

Exclusive distributor:

ORDERS

¯ By signing the order, the customer enters into a purchasing contract which Plexa S.r.l. will fulfil, if accepted, only in accordance with its contents.

¯ Prices are net of V.A.T.

¯ Orders of less than 200,000 lire net are not accepted.

¯ Plexa S.r.l. will only fulfil orders received by post or fax. Plexa

S.r.l. may draw up a ^confirmation of order~ at its own discretion.

¯ For transport procedure s, the purchaser must indicate the chosen means of shipment and the name of the carrier, or that he will collect the goods with his own vehicle.

¯ Delivery dates agreed are guideline and do not entitle the purchaser to cancel the order.

OFFERS, VALIDITY

¯ Any offers or order proposals drawn up by Plexa S.r.l. or its appointees are valid for 60 (sixty) days.

PAYMENTS

Plexa S.r.l. may permit the following types of payment.

¯ in cash or by cheque enclosed with the order (discount 5% in invoice);

¯ on delivery of the material (discount 5% in invoice);

¯ cash on delivery payable to carrier (discount 5% in invoice);

¯ bank payment order at 60 (sixty) days after invoice date with specific indication of the bank to be used.

¯ Any insolvency or delay in meeting agreed payment terms entitles

Plexa S.r.l. to suspend supply of goods in progre s s.

¯ Interest at the rate of 5% per annum above the prime rate will be charged on late payments.

WARRANTY

The material supplied is guaranteed for 12 (twelve) months after the date of delivery, against defects in materials or manufacture.

¯ Plexa S.r.l. undertakes to replace the faulty piece and/or repair it free of charge further to return to Plexa S.r.l. or its local Service

Centres in order to allow verification of the defect and the validity of the warranty.

¯ Faulty and replaced pieces are propriety of Plexa S.r.l.

¯ Any goods returned for replacement and/or repair during the warranty period must be consigned to Plexa S.r.l. or to its local

Service Centres freight prepaid, and will be returned to the customer with freight payable at destination.

¯ Labour will be charged at cost and then invoiced.

¯ Any acknowledgement of defects and/or no conformities in the goods sold shall not constitute any liability on the part of Plexa

S . r.l. and shall not constitute gro u n d s for a re q u e s t fo r compensation for damages by any title or through any action by the customer.

¯ The warranty becomes null and void if the material suplied by

Plexa S.r.l. is modified, used improperly and/or tampered with.

¯ S ystems must be constructed in accordance with the criteria s tated in law 46 dated 5 March 1990.

WORK BY TECHNICAL STAFF

¯ Work by internal technical staff on systems for any reason must be agreed in advance with Plexa S.r.l. and any invoices will be issued on the following conditions:

80.000 lire per hour for the duration of the work and travelling time of a system technician;

100.000 lire per hour for the duration of the work and travelling time of a sof t ware technician;

650 lire per kilometre for travel.

CLAIMS, COMPLAINTS AND RETURNS

¯ Any claims or complaints must be receive d, documented, by

Plexa S.r.l. or its local Service Centres within 8 (eight) days after the date of receipt of the material and do not constitute grounds for interruption of payments.

¯ Any returns must be agreed with and authorized by Plexa S.r.l.

in advance and must be made freight prepaid.

¯ A charge of 20% will be made for returns for which we are not responsible.

DELIVERY

¯ 30 (thirty) working days after the date of receipt of the order.

The term set is purely guideline and not binding.

TRANSPORT

¯ Goods travel at the purchaser´s risk, by means chosen by the purchaser and with expenses for his account, charged in the invoice if requested.

QUOTATIONS

¯ Plexa S.r.l. reserves the right to vary the price list (in whole or in part), informing its customers. The prices applied will be those of the price list in force when the order is placed.

DISCOUNTS

¯ Any discounts granted by Plexa S.r.l. appointees must be approved by the sales management before they are actually applied.

SUPPLY

¯ Plexa S.r.l. undertakes to supply the goods ordered with exclusion of assembly, installation and testing.

DISPUTES

¯ The Bologna Law Court has jurisdiction over any disputes.

IMPORTANT NOTES

¯ The magnetic card readers are supplied with ISO 2 track reading heads as standard. Specif the request of ISO 3 track reading head when ordering (extra charge).

¯ The PLW 760/T magnetic badges are supplied with ISO 2 track magnetic band, coded with low coercivity (300 Oe), conscutive numbering and punching in legible form (numbering equal to code), first 8 characters as standard. Specify reading track, coding, coercivity, punching different fro m s tandard w h e n ordering (extra charge).

¯ The PLW keypads used in systems with NET logic boards and terminals or PLW 380/MR decoders, have to be addressed by

Plexa before delivery depending on the use no extra charge).

¯ The reading distances stated in this documentation refer to tests performed in environments ideally free from disturbances and are therefore to be considered the maximum range in optimum conditions. Plexa S . r.l. tests all antennas produced in its works h o p s a n d t h e re fo re declines any responsibility fo r installation of antennas in places with sources of disturbance which may impair operation of the antennas.

¯ This price list annuls and replaces previous editions.

¯ (_®) Trademarks registered by their legitimate proprietors.

¯ All products based on Ticino Living_®, Vimar idea_® and Ave_® series mechanics are supplied without plaque.

¯ Plexa S.r.l. reserves the right to modify the data stated herein, even without notice.